# Caos

Power: 17W – 220/240Vac
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 1550lm (3000k) | 1700lm (4000k)
Optic: 120°

### Detailed Description

Indoor/Outdoor wall or ceiling LED device, made of anodized or painted aluminium and opal frontal screen.The LEDs used have a lifetime of 50.000hours under normal conditions of use as stated by the manufacturer.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension