# O Spot 10 narrow

10W
Power: 10 W – 24Vdc
Color temperature: 3000k (W)
Nominal flux: 1100lm (3000k)
Optic: da 8° fino a 60°

### Detailed Description

Up-light recessed luminaire with INOX steel turned ring. High-performing and flexible product. The circuit employed allows the instalment of 8° to 60° optics. Ideal either for high-bay lighting of spaces and surfaces or for creating strong contrasts.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension