# Trave Suspension

Design by FF Works

L.80cm
Power: 18+10W – 220/240Vac
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 2250+1327lm (3000k) | 2256+1365lm (4000k)
Optic: 32°

### Detailed Description

L.160cm
Power: 36+10W – 220/240Vac
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 4500+1327lm (3000k) | 5112+1365lm (4000k)
Optic: 32°

Suspension for direct and indirect light, born in combination with our TRAVE wall lamp. Modular suspension in various finishes with the possibility of choosing the various end pieces to match according to your preferences.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension