# O Spot 10

10W
Power: 10 W – 24Vdc
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 708lm (3000k) | 750lm (4000k)
Optic: 30° | 60°

### Detailed Description

10W
Power: 10W – 220/240Vac
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 1180lm (3000k) | 1250lm (4000k)
Optic: 30° | 60°

Up-light recessed luminaire with INOX steel turned ring. High-performing and flexible product. The circuit employed allows the instalment of 8° to 60° optics. Ideal either for high-bay lighting of spaces and surfaces or for creating strong contrasts.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension