# Oriente Trimless

Power: 25W – 700mA
Color Temperature: 3000k
Nominal flux: 2945lm
Optic: 20° | 30° | 50° | 75°

### Detailed Description

Painted aluminium recessed spotlight. Directional product, with an inclinationangle of maximum 25°, Product’s diameter: The recessed luminaire was designed to allow easy installation. The formworkcan be preliminarily levelled; the ring threading allows the successivetightening of the spotlight.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension