# Smart

Power:3W – 700mA | 24Vdc | 350mA RGB
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 325lm (3000k) | 360lm (4000k)
Optic: 360° | 180° | 90° | 90+90°

### Descrizione Dettagliata

Recessed 360°,180°,90°,90°+90° emitting LED footlight, made of stainless steel AISI 316 or natural bronze. Ideal for floating floors and covering up to 6mm thick. For thickness less than 6mm installable through specific wall-box. Drive over to maximum 1ton.

Datasheet

### Gallery

### Scopri le altre Categorie

#### Incassi

#### Paletti luminosi

#### Parete-Soffitto

#### Piscina

#### Proiettori

#### Illuminazione di facciate

#### Segnapasso

#### Sospensioni

#### Lettura