# Ghost

14W
Power: 14W – 220/240Vac
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 1624lm (3000k) | 1750lm (4000k)
Optic: 90°

### Detailed Description

25W
Power: 25W – 700mA
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 2900lm (3000k) | 3025lm (4000k)
Optic: 90°

Recessed LED device for indoor Ø100mm. Adapter Ø 180 mm with Opal lens Heatsink made of anodized aluminium and PMMA optic. When the product is turned off it is camouflaged with the ceiling, with a thickness of 3mm. A 90° lens of our design allows optimal distribution of light with a good visual comfort.

Datasheet

Electronic Brochure

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension