# Flute

H.30cm
Power:6W – 220/240Vac
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 612lm (3000k) | 678lm (4000k)
Optic: 36° | 80°

### Detailed Description

H.60cm
Power: 9W – 220/240Vac
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 1120lm (3000k) | 1356lm (4000k)
Optic: 36° | 80°

Indoor Pendant LED device with internal power supply. Body made of Anodized Aluminium and optic in PMMA.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension