# Pixel Maxi

Power: 15W – 350mA
Color Temperature: 3000k
Nominal Flux: 3x650lm
Optic: 16° | 30°

### Detailed Description

Downlight LED system 70x210mm with 3 sources 3W, adjustable to 350° with max inclination 90°. Made of Brilliant Black Anodized Aluminium, White lacquered and metacrylate. Ideal for lighting shop windows or display cabinets.

Datasheet
Datasheet single

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension