# Walker

Power: 3W – 700mA | 220/240Vac
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 325lm (3000k) | 360lm (4000k)
Optic: 80°

### Detailed Description

Indoor/Outdoor LED device. Available as wall footlight or ceiling spot.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension