# Reticolo 4

Power: 4W – 350mA
Color Temperature: 3000k
Nominal flux: 1026lm
Optic: 14° | 30° | 48°

### Detailed Description

Recessed LED spotlight with flange or trimless system. Black anodized aluminum body, painted flanges and polycarbonate optics. Possibility of creating continuous light lines. On request adjustable or double output version.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension