# Layer

Power: 18W – 220/240Vac
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 1872lm (3000k) | 1980lm (4000k)
Optic: Diffused

### Detailed Description

Indoor wall LED applique.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension