# Fuga

Power: 25W – 700mA
Color Temperature: 3000k
Nominal flux: 2905lm
Optic: 22° | 36° | 55° | 73°

### Detailed Description

Modular LED system. Designed for creating wall or ceiling joints. Painted galva-nized sheet metal case and aluminum spotlight with targeted optics.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension