# Pilz Uplight

Power: 3W – 700mA | 24Vdc | 220-240Vac
Color Temperature: 3000k
Nominal flux: 375lm
Optic: 12° | 30°

### Detailed Description

Anodised aluminium LED luminaire ideal for lighting gardens, with a turned body and up-light emission. Ideal product for lighting walls and ground applications, 30° e 60° optics available. Up-light emission. Supplied with formwork.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension