# Arco

Power: 6W – 220/240Vac
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 540lm (3000k) | 570lm (4000k)
Optic: 8×180°

### Detailed Description

LED device designed to be positioned in a window, door or walls corner to create light effects. Made of anodized aluminum with various finishes and proprietary PMMA lens technology.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension