# Lira

L.40cm (Medium)
Power: 7,5W – 24Vdc | 220/240Vac
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 1027lm (3000k) | 1117lm (4000k)
Optic: 15° | 32° | 15×44°

Below all the various options!

### Detailed Description

L.80cm (Medium)
Power: 15W – 24Vdc | 220/240Vac
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux 2145lm (3000k) | 2235lm (4000k)
Optic: 15° | 32° | 15×44°

L.120cm (Medium)
Power: 22,5W – 24Vdc | 220/240Vac
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 3217lm (3000k) | 3352lm (4000k)
Optic: 15° | 32° | 15×44°

L.40cm (High)
Power: 15W – 24Vdc | 220/240Vac
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 2144lm (3000k) | 2234lm (4000k)
Optic: 15° | 32° | 15×44°

L.80cm (High)
Power: 30W – 24Vdc | 220/240Vac
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 4290lm (3000k) | 4470lm (4000k)
Optic: 15° | 32° | 15×44°

L.120cm (High)
Power: 45W – 24Vdc | 220/240Vac
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 6434lm (3000k) | 6704lm (4000k)
Optic: 15° | 32° | 15×44°

For external use, in anodized aluminum and glass. Uses 24V dc, or with a special accessory “backpack”, connect directly to mains 220-240V. Possibility of dual emission and power in both the MEDIUM and HIGH version. The many available optics make this product extremely dynamic and responsive to different architectural requirements.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension