# Up&Down65

Power: 2×7,5W – 220/240Vac
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 885+885lm (3000k) | 937+937lm (4000k)
Optic: 24° | 36° | 48°

### Detailed Description

Indoor/Outdoor wall LED device, made of brass with internal dissipator made of aluminium. Available with optical 24°- 36°- 48° to high efficiency.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension