# Mini Q

Power 1.2 W – 350mA
Color temperature: 3000k (W)
Nominal flux: 135lm (3000k)
Optic: 16° | 90°

### Detailed Description

Recessed Mini Spot LED with square ring 30x30mm. Made of Anodized Aluminium Sink, Stainless steel or Bronze frame and PMMA lens. Available in ground recessed or plasterboard recessed.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension