# Domino 2 Ceiling

Power: 4W – 350mA
Color Temperature: 3000k
Nominal flux: 550lm
Optic: 8° | 30°

### Detailed Description

Ceiling lamp with anodised aluminium body. High efficacy circuit with various optics in order to optimize and precisely direct its light beam (available lenses 8°, 12°, 30°, EL).The module’s reduced dimension and the high efficacy circuit make the product extremely discreet and ideal for either accent or grazing illumination, wall-wash effect. We additionally foresee the possibility of integrating a honey comb filter inside the product.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension