# Iride

Power: 3W – 700mA | 24Vdc | 350mA RGB
5W – 350mA (turbo version)
Color Temperature: 3000k (W) | 4000k (N) | RGB (R)
Nominal flux: 375lm (3000k) | 426lm (4000k)
556lm (3000k) | 598lm (4000k) (turbo version)
Optic: 12° | 30°

### Detailed Description

Built-in swivel LED spot for indoor/outdoor. Made of stainless steel AISI316, bronze or white painted.
Available as uplight recessed into the ground or downlight on ceiling. The LEDs used have a lifespan of approximately 50,000 hours under normal conditions of use as declared by the manufacturer.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension