# Nubes

Design by Arch. Diego Collareda

25W
Power: 25W – 220/240Vac
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 2900lm (3000k) | 3025lm (4000k)
Optic: 60° | 120°

### Detailed Description

39W
Power: 39W – 220/240Vac
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 4292 (3000k) | 4477 (4000k)
Optic: 60° | 120°

Suspension lamp with integrated transformer. Ideal for lighting work premises. Prismatic screen for lighting areas with UGR <19 video terminals available on request.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension