# Side 100 150

Power: 14W – 700mA
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 1624lm (3000k) | 1750lm (4000k)
Optic: Asimmetrica°

### Detailed Description

Built-in swivel downlight LED with with asymmetrical bright beam with effect Wallwasher, Ø 100mm or Ø 150mm. Ring made of alluminium and polycarbonate optical reflector to high performance. LED CRI 90.

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension