# Step

Power: 1,1W -24Vdc
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 120lm (3000k) | 133lm (4000k)
Optic: 120°

### Detailed Description

Built-in swivel wall footlight side emitting, for indoor/outdoor, units can be painted to match the wall finishes.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension