# Round

Power: 1,2W – 350mA
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 150lm (3000k) | 170lm (4000k)
Optic: 360°

### Detailed Description

Built-in swivel wall footlights side emitting, for indoor/outdoor, paintable like the wall finish.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension