# Boomer 14

Power: 14W – 220/240Vac
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 1652lm (3000k) | 1750lm (4000k)
Optic: 14° | 26° | 45°

### Detailed Description

Track LED projector, balanced, adjustable with inclination max. 90°. Made of Aluminium and polycarbonate parables with antiglare screen. Available in ceiling version.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension