# Lira incasso

Power: 8W | 220/240Vac
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 1027lm (3000k) | 1117lm (4000k)
Optic: 15° | 32° | 15×44°

Below all the various options!

### Detailed Description

Floor recessed box 470 mm

Power: 15W
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 2145lm
Optic: 15° | 32° | 15×44°

Floor recessed box 837 mm

Power: 15W
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 2145lm
Optic: 15° | 32° | 15×44°

Floor recessed box 837 mm

Power: 30W
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 4290lm
Optic: 15° | 32° | 15×44°

Recessed LED profile made of Anodized aluminum and tempered glass. Ideal for wall-wash lighting effects. Available lengths and optics make this profile an extremely dynamic and responsive product in many architectural requirements.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension