# Up&Down40

Power: 2x3W – 700mA
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 375+375lm (3000k) | 426+426lm (4000k)
Optic: 12° | 30°

### Detailed Description

Indoor/Outdoor wall LED device, made of brass with internal dissipator made of aluminium.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension