# Traccia

100mm

Power: 3W
Color Temperature: 3000k
Nominal flux: 400lm (3000k)
Optic: 120°

### Detailed Description

Double Emission LED applique for indoor and outdoor. Made of painted alumi-nium and polycarbonate optic screen. Driver on board. Available in the catalog in 4 sizes. Suitable for ambient lighting.

200mm

Power: 6W
Color Temperature: 3000k
Nominal flux: 800lm (3000k)
Optic: 120°

400mm

Power: 12W
Color Temperature: 3000k
Nominal flux: 1600lm (3000k)
Optic: 120°

500mm

Power: 14W
Color Temperature: 3000k
Nominal flux: 1860lm (3000k)
Optic: 120°

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension