# Bulbus

Power: 7W – 350mA
Color Temperature: 3000k
Nominal Fux: 720lm
Optic: 360°

### Detailed Description

Is an alternative to the classic “bollards” or garden stakes format. It features a clean design with a strong personality. Illumination of 360 ° and an integrated power supply for 220/240 V. The light source concealed in the device is of very low luminance. The special lens in PMMA supplied with Bulbus is designed and produced in-house by Puraluce. Bulbus is also available with the special “Roots” system of Puraluce for anchoring in the ground. This system allows one to position the product at a desired height.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension