# Geco

14W
Power: 14W – 220/240Vac
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 950lm (3000k) | 1055lm (4000k)
Optic: 22° | 36° | 55° | 73°

### Detailed Description

25W
Power: 25W – 220/240Vac
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 2200lm (3000k) | 2350lm (4000k)
Optic: 22° | 36° | 55° | 73°

Spot in aluminum connected directly to mains (220-240Volt) for outdoor lighting in various shapes, different power output and different optics. t can also be used with a picket (ordered separately).

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension