# Smart Car

Power:3W – 700mA | 24Vdc | 350mA RGB
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 325lm (3000k) | 360lm (4000k)
Optic: 360° | 180° | 90° | 90+90°

### Detailed Description

Recessed 360°,180°,90°,90°+90° emitting LED footlight, made of stainless steel AISI 316 and natural bronze. Drive over to maximum 3,5 tons.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension