# Etna Wall

Radial
Power: 7W – 220/240Vac
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 826lm (3000k) | 875lm (4000k)
Optic: 360°

### Detailed Description

single side light beam 180°
Power: 7W – 220/240Vac
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 826lm (3000k) | 875lm (4000k)
Optic: 180°

Indoor/Outdoor wall LED device, radial beam 360° or single side light beam 180°, made of anodized aluminium or natural copper and clear methacrylate optic.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension