# Giunto Ceiling

Design by 997 architecture

20x20cm
Power: 25W – 220/240Vac
Color Temperature: 3000k
Nominal flux: 2905lm
Optic: Diffused

### Detailed Description

40x40cm
Power: 60W – 220/240Vac
Color Temperature: 3000k
Nominal flux: 7020lm
Optic: Diffused

LED ceiling lamp, made of painted Aluminium and opal or prismatic screen. Available with dynamic adjustment of light intensity and Kelvin temperature. Also available in two size, 220x220mm e 620x620mm.

Electronic Brochure
Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension