# 48Vdc Continuous Line

Length: 600mm
Pwer: 12W – 48Vdc
Color Temperature: 3000k
Nominal flux: 1292lm
Optic: Diffusa

### Detailed Description

Length: 900mm
Power: 19W – 48Vdc
Color Temperature: 3000k
Nominal flux: 2068lm
Optic: Diffusa

Length: 1900mm
Power: 43W – 48Vdc
Color Temperature: 3000k
Nominal flux: 4680lm
Optic: Diffusa

Continuous line for 48Vdc electrified tracks. Anodized aluminum body and opal cover.

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension