# Deep mini

Version Mini 6cm
Power: 14W – 350mA |
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 1652lm (3000k) | 1750lm (4000k)
Optic: 24°

### Detailed Description

Version Standard 8cm
Power:25W – 700mA | 220/240Vac
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 2900lm (3000k) | 3025lm (4000k)
Optic: 22°

DEEP is a recessed spotlight, with recessed LED source for maximum viewing comfort. It illuminates while concealing the light source. he spotlight DEEP, with its “bull’s eye” effect, concentrates the luminance on the underlying objects, obtaining excellent “theatrical” effects. Realized in aluminum and polycarbonate reflectors with clear or antiglare screen.

Electronic Brochure

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension