# Lucciola

Power: 3W – 24Vdc | 220/240Vac
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 325lm (3000k) | 360lm (4000k)
Optic: 12° | 30°

### Detailed Description

Small spotlight in aluminum, 24 VDC for exterior lighting, but also suitable for interior use. Available with a variety of finishes and optics. It can also be used with a picket (ordered separately). vailable with a variety of finishes and optics. On request also available with lenses 8 °,18 °,58 °,44×10°.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension