# Giunto

Design by 997 architecture

Power: 25W – 220/240Vac
Color Temperature: 3000k
Nominal flux: 2905lm
Optic: Diffusa

### Detailed Description

LED wall lamp, made of painted Aluminium and opal or prismatic screen. Available with dynamic adjustment of light intensity and Kelvin temperature. The modular concept of the device allows you to vary the combination of surface material according to the type of application.

Electronic Brochure
Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension