# Leddi

Power: 3W – 100/240Vac 50~60Hz
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 375lm (3000k) | 426lm (4000k)
Optic: 30°

### Detailed Description

Independent wall reading lamp with switch. Electronic transformer integrated.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension