# Gemini

Power: 14W – 700mA (CC) | 220/240Vac (HI)
Color Temperature: 3000k (W) | 4000k (N)
Nominal Flux: 2010lm (3000k) | 2220lm (4000k)
Optic: 120°

### Detailed Description

Modular wall lamp in anodized aluminum or painted in various finishes. Available in three versions, Right, Left,and Central.

Datasheet

### Gallery

### Discover the other Categories

#### Recessed Light

#### Reading

#### Bollard

#### Wall – Ceiling

#### Pool

#### Projector

#### Facades Lighting

#### Footlight

#### Suspension